

**Technical Specifications Theaters Tilburg Studiozaal**

**Address**

City Tilburg

Theatre Theaters Tilburg

Hall Studio Tilburg

Visiting address Louis Bouwmeesterplein 1

Postal code/City 5038 TN Tilburg

Loadingdock across from Schouwburgring 51

Postaddress Postbus 3035

Postal code/City 5003 DA Tilburg

**Telephone**

Ticket shop +31 13 543 22 20

General +31 13 549 03 90

E‐mail techniek@theaterstilburg.nl

**Personal data**

Technical coordination Pernel van Herpt +31 13 549 03 28
Ineke Padmos +31 13 549 03 27 techniek@theaterstilburg.nl

Production Anne Rosenau +31 13 549 03 16 arosenau@theaterstilburg.nl

 **Standard working hours**
Lunch 12:30 ‐ 13:00
Diner 17:30 ‐ 19:30

Showtime evening : 20:30 / matinée 14:00
Opening hours green room: in consultation
Booth open between 17:30 and 19:30: in consultation

**Parking/Accessibility**Note:since 2010 the Schouwburgring is one way only
Access: good (see map and directions)
Parking trucks/cars: in consultation

**Loading dock**Details: the studio is 3 meters below street level.
All goods are transported by an elevator. The car is parked on the pavement during the load in and load out and must be parked somewhere else afterwards. There is no roof.

Elevator dimensions: L 4.00 m X W 1.20 m X H 2.10 m
Capacity: 1500 kg

Smallest passage to stage and dressing rooms:
Width: 1.20 m
Height: 2.00 m

**Sound**Fixed installation:Mixer: SD 1132 Input Channels, 8 x 8 Full Processing Matrix, 4 Dynamic Equalizers, 4 Multiband compressors, 4 Digital FXSound equipment:Amplifiers: powersoft M50Q, M30D, 3904Speakers: Martin Audio XD12/S18DSP system: Peavey MM NionMonitorsAmplifier D6Speakers 2-max 12

**Peripherals**Besides the fixed installation Theaters Tilburg has a fairly wide range of mixers, microphones, transmitters, effects, monitors and other peripherals with sufficient wiring.

In consultation per room available. For information and availability please contact the technical department.

Sound booth: yes

Monitoring : DSP FOH

Open window possible: yes

Sound seats in room: yes

Position sound seats: behind in the middle

Clean power on stage: yes, 1 x 16 A

Clean power in room: yes, 1 x 16 A

Clean power in booth: yes, 1 x 16 A

**Light**

Light booth

Position of light booth: behind in the middle of the room

Light console: Road Hog 4

Space for console of visiting party: yes

Open window possible: yes (no colored glass)

Remote: yes compucall/iPad

Light console portable: Road hog 4 is portable

House lights controlled by DMX: yes

 **Lighting equipment:**

**Fixed materials**

Position Amount Type Power Make Angle Barndoors

Plan 1 8 P.C. 650w ADB A56C 9-66° 45°/90° yes

Plan 2 6 P.C. 650w ADB A56C 9-66° 45°/90° yes

Plan 3 6 P.C. 650w ADB A56C 9-66° 45°/90° yes

Plan 4 8 P.C. 650w ADB C52 9-60° 75°/90° yes

Cyclorama 12 4 Cyclorama units 500w Strand coda 500/4 45° above and underneath

**Loose Materials**

Amount Type Power Make Type Angle Barndoors

12 P.C. 650w ADB C52 9-60° 75°/90° yes

20 Zoom Profile 600 w Selecon Pacific 23° / 50° n.a.

24 Par Source Four 575 w ETC EU 4 lenses

4 Ballet towers

Plug material: cee 16/32/63/125 A + shuko
Main Power: Distance to stage
Stage right 63 A Cee 7.00 m (standard : floor dimmer and the cyclorama units connected to it) Stage left: 63 A
Sound seats: 1 x 32 Amp Cee 15.00 m
Foyer: 2 x 32 A

**Details:**

Dimmerprotocol: DMX

Connector type: 5 way XLR

Dimmers connectable to visiting parties console: yes

Extra DMX connections: male female

**Dimensions / Seats**

The theater is 3.96 meter high, this is measured from floor to bottom grid. The lamps and speakers are hanging below.

The stage floor is 14 meters wide using side black and 8 to 12 meters wide using legs.

Maximum amount of chairs: 250 (always after consult)

Stage 5,0 m depth: 185 chairs (4 rows before seating system)
Stage 6,0 m depth: 165 chairs (3 rows before seating system)
Stage 7,0 m depth: 145 chairs (2 rows before seating system)
Stage 7,5 m depth: 130 chairs (1 row before seating system)
Stage 8,0 m depth: 110 chairs (seating system only)

These setups are including 2 x 4 sound seats.
No seats and no drapery/masking: 570 people can stand in the room

Theatre type: Flat stage (black box, flat stage, variable, podiumhall)
Year of construction: 1961
Renovation: 2002 (involved: dressing rooms, loading dock)

 **Drapery/Masking**

Description Amount High Wide Color: Material: Rail:

Legs 2 x 5 4.00 m X 3.50 m dark blue velours yes

Cyclorama 1 4.00 m X 14.00 m white cotton yes

Border 1 4.00 m X 12.00 m dark blue velours yes

Side tabs 2 X 3 4.00 m X 3.50 m dark blue velours yes

Back wall: Plaster wall with an angle, the color of the hall is dark blue
Ballet Floor available: yes 10.00 meters wide. Black / white (the white side is not very clean).
Wooden floor, angle 0

**Grand Piano**
Yamaha C3 x

**Piano**
Seiler

**Dressing rooms**

There are two dressing rooms: suitable for 5 people
Equipped with: make-up mirror, sink, stage sound.
Only one dressing room with shower

Call to: public spaces and dressing rooms

Details:
Washer and dryer connections in the dressing room corridor of the schouwburg.
The studio does not have a green room. If there is a show in the schouwburg, then the green room will be opened from 18:30 pm. Otherwise in consultation.

**Connections**

Cable TV jack: Yes distance from the stage (m): 15.00 m

Internet: yes distance from the stage (m): 15.00 m

Wireless Internet: In the dressingrooms and public area

Hose: yes Location: salvage

Crane and drainage: yes, side stage at the bar

Smoke detector: yes, can be disabled: to be negotiated

Ventilation in the room switched off: no

Light is adjusted with a self-propelled platform

Intercom: master station in the control room

Connection for additional intercom stations: control room, dressing room, stage left and stage right